### Firmware Version(v0.23):

        - 4NV7B.bin: DJN-15-22511, 4inch, driver board: V05/V07
        - 4NV10B.bin: TOSHIBA(screen with an "ear"), 4inch, driver board: V10
        - 5NV7B.bin: SLM5.0-81FPC-A, 5inch, driver board: V07
        - 4N3V7B.bin: D430FPC9316-A, 4.3inch, driver board: V07
        - 4NDXV7P.bin: D397FPC9367-B, 4inch, driver board: V07
        - 5NDV7B.bin: D500FPC9373-G, 5inch, driver board: V07
        - 7NDV7B.bin: D680FPC930G-A, 6.8nch, driver board: V07
        - 7NDV7B.rpi.bin: D680FPC930G-A, 6.8nch, driver board: V07 (RaspberryPi version)
        
        - MPROT.5d0.VOCORE.bin: D500FPC931A-A, 5inch, driver board: MPRO
	- MPROT.3r4.VOCORE.bin: VOCORE-3.4IN-ROUND, 3.4inch round, driver board: MPRO
	- MPROT.4d0.VOCORE.bin: VOCORE-4.0INRGB, 4.0inch, driver board: MPRO
	- MPROT.4d3.VOCORE.bin: VOCORE-4.3INRGB, 4.3inch, driver board: MPRO
	- MPROT.6d8.VOCORE.bin: VOCORE-6.8INRGB, 6.8inch, driver board: MPRO
	- MPROT.10d.VOCORE.bin: VOCORE-10INRGB, 10inch, driver board: MPRO
	- for no logo firmware, please use MPROT.xxx.NOLOGO.bin
	- MPROT: logo at top side, MPROB: logo at bottom side

### LVGL DEMO Firmware
        - MPRO.4s0.LVGL.bin: D395FPC2503-A, 4.0inch square, driver board: MPRO

Warning: using wrong firmware will lock or break the screen!!! If bricked please contact support@vocore.io
Please use v2scrctl and choose correct firmware version for your screen, use "Upgrade" to load firmware.
